ALARM CROSSWORD PUZZLE

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  | 1 |  |  |  | 2 |  |  |  | 3 |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  | 4 |  |  |  |  |  | 5 |  |  |  |  |  | 6 |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 7 |  |  |  | 8 |  |  |  | 9 |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 10 |  |  |  |  |  | 11 |  |  |  |  | 12 |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  | 13 |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  | 14 |  |  |  |  |  |
|  |  |  |  | 15 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 16 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  | 17 |  |  |  |  |  |  | 18 |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 19 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| **Across****5.** This device is only installed at telling positions where a camera is installed and is titled \_\_\_\_\_ suspicious button.**7.** ,Which device is ceiling mounted 3 metres inside the main entry door.**9.** This device performs five distinct functions 1. green light - hold-up pre alarm 2. red light - hold-up activated 3. blue light - back door activated 4. siren will sound 5. the red button is also a hold up activator**11.** System \_\_\_\_\_\_ are placed in the following areas 1. front entry 2.banking chamber 3. information desk 4. public**13.** Staff are issued a personal identification number to access this \_\_\_\_\_\_\_.**15.** What does DOTL stand for?**16.** Both HUA \_\_\_\_\_\_ depressed together generate an alarm with the standard 60 second delay**17.** The safe reed switch is designed to ensure that \_\_\_\_\_ and safes are not left in the open position when the system is full night seal.**18.**  Front entry doors are not covered by a \_\_\_\_\_ this is to allow couriers to deliver the mail bags inside the front area with out the requirement of a code.**19.** The main RAS is wall mounted in the back of the house area, typically in close proximity to the main \_\_\_\_\_\_\_\_\_ or vault. | **Down****1.** What does RAS stand for?**2.** What does AIP stand for?**3.** What does HUA stand for?**4.** What light illuminates when it tell you to not move beyond this point until advised to do so by front of house staff**6.** ,This device is installed at all workstations in the branch when pressed once it activate a hold-up alarm 60 seconds after activation , multiple activation will activate a hold-up alarm immediately**8.** this alarm is positioned throughout the branch ,ceiling mounted this device is used for the timer ending on challenger**10.** 10 inch and 12 inch \_\_\_\_\_\_\_ are positioned within the branch mostly in a general area for viewing and monitoring.**12.**  Service crews attending the site hold a master key for these boxes.**14.** The ROT will emit an unusual ringing when a \_\_\_\_\_\_\_\_\_\_\_\_ button has been activated |