|  |  |
| --- | --- |
| Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

Fall Protection - Safety Awareness Month

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  | 1D |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  E |  | 2S |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  S |  |  H |  |  |  |  |  |  |  |  |
|  |  |  | 3C |  |  |  | 4D |  |  C |  |  O |  | 5R |  |  |  |  |  |  |
|  | 6O |  |  O |  |  |  |  A |  |  E |  |  C |  |  E |  |  |  |  |  |  |
|  |  V |  |  M |  |  |  |  M |  |  N |  |  K |  |  P |  |  |  |  |  |  |
|  |  E |  |  P |  | 7G |  U |  A |  R |  D |  R |  A |  I |  L |  S |  |  |  |  | 8E |
|  |  R |  |  E |  |  |  |  G |  |  |  |  B |  |  A |  |  | 9W |  |  |  Q |
|  |  R |  |  T |  |  |  |  E |  |  |  | 10S |  E |  C |  U |  R |  E |  D |  |  U |
|  |  E |  |  E |  |  |  |  D |  | 11T |  |  O |  |  E |  |  |  I |  |  |  I |
| 12H |  A |  R |  N |  E |  S |  S |  | 13T |  H |  I |  R |  D |  |  |  |  G |  |  |  P |
|  |  C |  |  T |  |  |  |  |  |  R |  |  B |  |  |  |  |  H |  |  |  M |
|  |  H |  |  |  | 14T |  H |  R |  E |  E |  |  E |  | 15B |  E |  L |  T |  |  |  E |
|  |  I |  |  |  |  |  |  |  |  E |  |  R |  |  |  |  |  |  |  |  N |
|  |  N |  | 16S |  | 17J |  U |  M |  P |  |  | 18S |  T | 19O |  P |  |  |  |  |  T |
|  |  G |  |  O |  |  |  |  |  |  |  |  |  |  S |  |  |  |  |  |  |
|  |  |  |  L |  |  |  |  |  |  |  |  |  |  H |  |  |  |  |  |  |
|  |  | 20S |  I |  D |  E |  R |  A |  I |  L |  S |  | 21F |  A |  L |  L | 22S |  |  |  |
|  |  |  |  D |  |  |  |  |  |  |  |  |  |  |  |  |  I |  |  |  |
|  |  |  |  |  |  |  | 23P |  R |  E |  V |  E |  N |  T |  |  |  X |  |  |  |

|  |  |
| --- | --- |
| **Across****7.** Railings designed to minimize fall risk at a work site where there is high fall risk.**10.** Lanyards must be? **12.** In the event of a fall, what distributes the fall arrest force over the pelvis, thighs, waist and shoulders? **13.** Don't stand higher than the \_\_\_\_\_ rung from the top of a ladder.**14.** Portable ladders need to be positioned to the side rails and extend at least \_\_\_\_\_\_\_feet above the landing. **15.** Use a tool \_\_\_\_ when climbing instead of carrying tools in your hand. **17.** Don't \_\_\_\_\_ off a ladder. **18.** Personal fall arrest systems must bring an employee to a complete what? **20.** When climbing a ladder, always face it and grip the rungs, not the \_\_\_\_\_\_\_. **21.** The leading cause of death for construction employees**23.** Proper ladder setup will help \_\_\_\_\_\_\_\_\_ slips and falls whether at home or work.  | **Down****1.** If the weather turns bad when you are climbing, \_\_\_\_\_\_\_ immediately. **2.** If the arresting forces of the lanyard alone can cause injury you must use these**3.** What type of person should inspect equipment annually? **4.** Never use a \_\_\_\_\_ ladder. **5.** What you do with equipment that has been involved in a fall?**6.** Instead of leaning or \_\_\_\_\_\_\_\_, repositioning the ladder closer to the work you are doing. **8.** Needs to be inspected daily**9.** Make sure you know the \_\_\_\_\_ limits of the ladder you are using. **11.** Always keep at least \_\_\_\_\_ points of contact with a ladder. **16.** Place the base of a ladder on a firm\_\_\_\_\_ surface. **19.** Use only ladders that comply with what standards?**22.** Fall protection is required when working at or above how many feet per OSHA |