|  |  |
| --- | --- |
| Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

Net wrk administration

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | 1 |  |  |  |  |  |  |  |  |  |  |
|  | 2 |  |  |  |  |  |  |  |  |  |  |  | 3 |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  | 4 |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 5 |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 6 |  |  |  | 7 |  |  | 8 |  |
|  | 9 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  | 10 |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 11 |  | 12 |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 13 | 14 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  | 15 |  |  |  |  |  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| **Across**  **2.** appliance (a combination of hardware and software) or an application (software) designed to control the flow of Internet Protocol (IP) traffic to or from a network or electronic equipment.  **4.** Central NAT can be disabled from?  **6.** Network adress Translation  **10.** Type\_\_\_\_\_\_\_\_\_\_\_\_\_\_associates an internal IP with a pool IP on a first-come, first-served basis  **11.** The User Datagram Protocol  **13.** Type\_\_\_\_\_\_\_associates an internal IP range with an external IP range  **15.** table enables you to define, and control with more granularity, the address translation performed by the FortiGate unit. | **Down**  **1.** Enabling\_\_\_\_\_\_\_\_\_changes Destination NAT configuration  **3.** Central Processing Unit  **5.** Source Network Address Translation  **7.** Default type is  **8.** a unique string of numbers separated by periods that identifies each computer using the Internet Protocol to communicate over a network.  **9.** Once enabled, can configure from\_\_\_\_\_\_\_  **12.** Port Address Translation  **14.** Internet Control Message rotocol |