|  |  |
| --- | --- |
| Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

Activity:Crossword Puzzle

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  | 1 |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 2 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  | 3 |  |  |  |  |  |  |  |  |  |
|  | 4 | 5 |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 6 |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 7 |  |  |  |  |  | 8 |  |  |  |  |
|  |  |  |  | 9 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 11 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  | 12 |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 13 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 14 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| **Across****1.** Range of frequency over which signals are equally amplified \_\_\_\_\_\_\_\_\_\_**4.** When two different signals(Out of phase) then mode is \_\_\_\_\_\_\_\_\_\_\_**7.** Change in Offset Voltage wrt change in Power Supply Voltage is \_\_\_\_\_\_**10.** Maximum Rate of change of output voltage is \_\_\_\_\_\_\_\_\_\_\_**11.** Voltage applied at the input to nullify the error voltage at output \_\_\_\_**12.** Ideal value of \_\_\_\_\_\_\_\_\_\_ Resistance in OP AMP is Zero**13.** When one of the terminal is grounded and signal is applied to other terminal is \_\_\_\_\_\_\_\_\_\_ Mode**14.** In the Block diagram of OP AMP \_\_\_\_\_\_\_\_ stage brings the DC level to Zero wrt ground | **Down****2.** The ratio of differential Gain to Common Mode gain is called \_\_\_\_\_\_\_**3.** Average value of two input currents in OP Amp is \_\_\_\_\_\_\_\_\_**5.** Ideal Value of \_\_\_\_\_\_\_\_ resistance is infinity**6.** Mode in which Phase, Frequency and Amplitude of Signals applied to 2 inputs **8.** Difference of two input currents in OP AMP is \_\_\_\_\_\_\_\_\_**9.** Operational Amplifier is also called as\_\_\_\_\_\_\_\_\_ |