|  |  |
| --- | --- |
| Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

Fall Protection - Safety Awareness Month

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  | 1  D |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  | E |  | 2  S |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  | S |  | H |  |  |  |  |  |  |  |  |
|  |  |  | 3  C |  |  |  | 4  D |  | C |  | O |  | 5  R |  |  |  |  |  |  |
|  | 6  O |  | O |  |  |  | A |  | E |  | C |  | E |  |  |  |  |  |  |
|  | V |  | M |  |  |  | M |  | N |  | K |  | P |  |  |  |  |  |  |
|  | E |  | P |  | 7  G | U | A | R | D | R | A | I | L | S |  |  |  |  | 8  E |
|  | R |  | E |  |  |  | G |  |  |  | B |  | A |  |  | 9  W |  |  | Q |
|  | R |  | T |  |  |  | E |  |  |  | 10  S | E | C | U | R | E | D |  | U |
|  | E |  | E |  |  |  | D |  | 11  T |  | O |  | E |  |  | I |  |  | I |
| 12  H | A | R | N | E | S | S |  | 13  T | H | I | R | D |  |  |  | G |  |  | P |
|  | C |  | T |  |  |  |  |  | R |  | B |  |  |  |  | H |  |  | M |
|  | H |  |  |  | 14  T | H | R | E | E |  | E |  | 15  B | E | L | T |  |  | E |
|  | I |  |  |  |  |  |  |  | E |  | R |  |  |  |  |  |  |  | N |
|  | N |  | 16  S |  | 17  J | U | M | P |  |  | 18  S | T | 19  O | P |  |  |  |  | T |
|  | G |  | O |  |  |  |  |  |  |  |  |  | S |  |  |  |  |  |  |
|  |  |  | L |  |  |  |  |  |  |  |  |  | H |  |  |  |  |  |  |
|  |  | 20  S | I | D | E | R | A | I | L | S |  | 21  F | A | L | L | 22  S |  |  |  |
|  |  |  | D |  |  |  |  |  |  |  |  |  |  |  |  | I |  |  |  |
|  |  |  |  |  |  |  | 23  P | R | E | V | E | N | T |  |  | X |  |  |  |

|  |  |
| --- | --- |
| **Across**  **7.** Railings designed to minimize fall risk at a work site where there is high fall risk.  **10.** Lanyards must be?  **12.** In the event of a fall, what distributes the fall arrest force over the pelvis, thighs, waist and shoulders?  **13.** Don't stand higher than the \_\_\_\_\_ rung from the top of a ladder.  **14.** Portable ladders need to be positioned to the side rails and extend at least \_\_\_\_\_\_\_feet above the landing.  **15.** Use a tool \_\_\_\_ when climbing instead of carrying tools in your hand.  **17.** Don't \_\_\_\_\_ off a ladder.  **18.** Personal fall arrest systems must bring an employee to a complete what?  **20.** When climbing a ladder, always face it and grip the rungs, not the \_\_\_\_\_\_\_.  **21.** The leading cause of death for construction employees  **23.** Proper ladder setup will help \_\_\_\_\_\_\_\_\_ slips and falls whether at home or work. | **Down**  **1.** If the weather turns bad when you are climbing, \_\_\_\_\_\_\_ immediately.  **2.** If the arresting forces of the lanyard alone can cause injury you must use these  **3.** What type of person should inspect equipment annually?  **4.** Never use a \_\_\_\_\_ ladder.  **5.** What you do with equipment that has been involved in a fall?  **6.** Instead of leaning or \_\_\_\_\_\_\_\_, repositioning the ladder closer to the work you are doing.  **8.** Needs to be inspected daily  **9.** Make sure you know the \_\_\_\_\_ limits of the ladder you are using.  **11.** Always keep at least \_\_\_\_\_ points of contact with a ladder.  **16.** Place the base of a ladder on a firm\_\_\_\_\_ surface.  **19.** Use only ladders that comply with what standards?  **22.** Fall protection is required when working at or above how many feet per OSHA |