|  |  |
| --- | --- |
| Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

ITD Tools and Equipment

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  | 1 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  | 2 |  | 3 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 4 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 5 |  |  |  |  |  |  |  |  |  |  |  |  | 6 |  |  |  |  |  |  |
|  |  |  |  |  |  | 7 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 8 |  | 9 |  |  |
|  |  |  |  |  |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  | 11 |  | 12 |  |  |  |  |  |  | 13 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  | 14 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  | 15 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  | 16 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 17 |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 18 |  |  |  |  |  |  |  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| **Across****1.** USED FOR STRAIGHT CUTS IN TIMBER.**4.** FOR PUNCHING/DRIVING NAILS BELOW THE TIMBER SURFACE; USED WITH A HAMMER.**7.** USED FOR CURVED CUTS IN TIMBER.**10.** EQUIPMENT USED FOR SMOOTHING TIMBER IN A CIRCULAR DIRECTION**12.** USED TO CUT SHEETMETAL**14.** USED TO MARK EVEN LINES PARALLEL TO AN EDGE OF SHEETMETAL**15.** A PEDESTAL STATION USED FOR DRILLING.**16.** USED TO HIT PUNCHES ON METAL SURFACES**17.** USED TO MAKE SMALL INDENTATIONS IN METAL. **18.** SET AT 90° FOR DRAWING ON TIMBER SURFACES AND CHECKING RIGHT ANGLES ON PROJECTS. | **Down****2.** EQUIPMENT USED TO NEATLY FOLD LONG PIECES OF SHEETMETAL**3.** USED TO DRIVE AND REMOVE NAILS INTO TIMBER SURFACES.**5.** FOR FINE/SMALL (10-20MM BRADS) NAILING WORK IN TIMBER SURFACES.**6.** USED TO REMOVE WASTE MATERIAL AND/OR SMOOTH EDGES OF METAL AND ACRYLIC**8.** USED TO FOLD OVER THE EDGES OF SHEETMETAL ON A STAKE**9.** USED TO MARK LINES ON METAL SURFACES**11.** USED WITH A DRESSER TO MAKE FOLDS ON SHEETMETAL**13.** USED TO MAKE SMALL HOLES IN SHEETMETAL FOR RIVETS. |