|  |  |
| --- | --- |
| Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

Lighting for the Stage

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  | 1 |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  | 2 |  |  |  |  |  |  |  | 3 |
|  |  |  |  |  |  |  |  |  |  | 4 |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  | 5 |  |  |  | 6 |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 7 |  |  |
|  |  |  |  |  |  |  |  | 8 |  |  |  |  |  |  |  |  |  |  |  |
|  | 9 |  |  |  |  |  | 10 |  |  |  |  |  |  |  | 11 |  |  |  |  |
|  |  |  | 12 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  | 13 |  |  |  | 14 |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  | 15 |  |  |  |  |  |  |
| 16 |  |  |  |  |  |  |  |  |  |  |  | 17 |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 18 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| **Across**  **2.** Type of lantern which produces an intense beam of light.  **6.** When all the lanterns in the rig are angled in the correct direction, and have their beam of light defined.  **10.** A rotatable attachment consisting of two or four metal flaps (hinged) which is fixed to the front of a Fresnel or PC type lantern to cut off the beam in a particular direction(s).  **13.** The type of material used to create colours in some lights.  **14.** Type of light that can be programed to create lots of colours using the different settings.  **16.** The direction given when you walk to the front of the stage.  **17.** Wiring, temporarily rigged, to carry electrical current.  **18.** When you are standing on the other side of the stage. | **Down**  **1.** A framework of alloy bars and triangular cross-bracing providing a rigid structure, particularly useful for hanging lights where no permanent facility is available.  **3.** Adding or subtracting to create colours  **4.** Each instrument is capable of a massive variety of effects which are operated live via a moving light control desk, or can be pre-programmed by a standard memory lighting desk.  **5.** Light coming from upstage, behind scenery or actors, to sculpt and separate them from the background  **7.** The direction given when you go to the back of the stage.  **8.** An increase, diminishment or change in lighting  **9.** Complete absence of stage lighting.  **11.** When you are standing on the side of the stage.  **12.** A type of lantern which produces an even, soft-edged beam of light through this type of lens.  **15.** The horizontal metal (steel or alloy) tube hung from flying lines (or forming part of a grid) from which lighting equipment and scenery etc. may be suspended. |

   Bar       Barndoors       Blackout       Backlight       Colourmixing       Downstage       Upstage       Cable       Fade       Focus       Fresnel       Gel       LED       Movinghead       Parcan       Stage left       Stageright       Truss