|  |  |
| --- | --- |
| Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

Plumbing Crossword Puzzle

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | 1 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 2 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  | 3 |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  | 4 |  |  |  | 5 |  |
|  |  |  |  | 6 |  | 7 |  |  |  |  |  | 8 |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 9 |  |  |  |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 11 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  | 12 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  | 13 |  |  |  |  |  |  |  |  |  |  | 14 |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  | 15 |  |  |  |  |  |  | 16 |  | 17 |  |  |  |
|  |  |  |  |  |  | 18 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  | 19 |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  | 20 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| **Across****2.** Type of wrench that has self-cleaning threads with interchangeable hook and heel jaws (two words)**7.** Changes the angel or direction of the flow without bending the pipes**8.** Used when you want to shut off the water since it stops the flow of water**9.** Enables the release of sewer gases outside instead of inside the home**10.** Type of pipe mostly found in homes that are composed of PVC or CPVC**12.** Turn this off prior to working on plumbing jobs around electrical wires (two words)**13.** PVC pipes are joined together using this adhesive (two words)**14.** Bend in the pipe near the fixture that holds or traps water**15.** Used to connect pipes**17.** Always wear \_\_\_\_\_\_\_ when working on a plumbing job**19.** Waste or sewer lines require a \_\_\_\_\_\_\_\_\_ percent slope**20.** Work that happens after interior finishing, like drywall and flooring (two words) | **Down****1.** The point in the ground where the pipes will not freeze in the winter (two words)**3.** A \_\_\_\_\_\_ \_\_\_\_\_\_ \_\_\_\_\_\_ heats the water in a home**4.** Tool with a rubber suction cup and attached stick used to clear blockages in drains and pipes**5.** Tool used to dislodge clogs (two words)**6.** A \_\_\_\_\_\_\_\_ is located on all properties and calculates how much water is being used. **11.** Cutting tool with replaceable blades used to cut large plastic pipes.**16.** Once water is used, it is sent down a drain and disposed through a sewage system or \_\_\_\_\_\_\_\_\_\_\_\_\_ system**18.** type of wrench used in confined spaces to turn fasteners that would be difficult or impossible to reach with a plumber wrench |