|  |  |
| --- | --- |
| Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

Preventing Forklift Accidents

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  | 1  S | E | A | T | B | E | L | T | S |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  | 2  O | V | E | R | H | E | A | D |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  | 3  B |  |  |  |  |  |  |  |
|  |  |  |  |  | 4  P |  |  |  |  |  |  | A |  |  | 5  P |  |  |  |  |
|  |  |  |  |  | E |  |  |  |  | 6  T |  | C |  |  | A |  |  |  |  |
|  | 7  I | N | S | I | D | E |  |  | 8  F | O | R | K | S |  | 9  S | L | O | W |  |
|  |  |  |  |  | E |  |  |  |  | P |  |  |  |  | S |  |  |  |  |
|  |  |  |  |  | S |  |  | 10  F |  | H |  |  |  |  | E |  |  |  |  |
|  |  |  | 11  R |  | T |  | 12  W | I | D | E |  | 13  H | O | R | N |  |  |  |  |
|  |  |  | E |  | R |  |  | V |  | A |  |  |  |  | G |  |  |  |  |
|  |  | 14  B | A | L | A | N | C | E |  | V |  |  |  |  | E |  |  |  |  |
|  |  |  | R |  | I |  |  |  |  | Y |  |  |  |  | R |  |  |  |  |
|  |  |  |  |  | N |  |  | 15  B |  |  |  |  |  |  | S |  |  |  |  |
|  |  |  |  |  | 16  S | T | R | A | I | G | H | T |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  | C |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  | K |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  | U |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  | 17  I | N | S | P | E | C | T | E | D |  |  |  |  |  |  |

|  |  |
| --- | --- |
| **Across**  **1.** Drivers should always wear \_\_\_\_\_\_.  **2.** All rider forklifts must have an \_\_\_\_ guard to protect the operator from falling objects.  **7.** The driver should keep hands, arms, and legs \_\_\_\_ in case of a tipover.  **8.** No one should be allowed to stand or pass under the \_\_\_\_\_.  **9.** Operators should \_\_\_\_\_\_ down and sound the horn at intersections and when entering the shop.  **12.** The back of a forklift swings \_\_\_\_\_ on a turn.  **13.** Drivers need to sound the \_\_\_\_\_ blind corners, doorways and aisles.  **14.** Sharp or sudden turns can throw a forklift off \_\_\_\_\_\_\_.  **16.** Forklifts should travel only \_\_\_\_ up and down a grade.  **17.** Forklifts must be \_\_\_\_\_\_\_before each shift. | **Down**  **3.** Loads should be placed as far \_\_\_\_\_ as possible for extra stability.  **4.** Almost one out of five fatal accidents kill other workers or \_\_\_\_\_.  **5.** Drivers should never carry \_\_\_\_\_\_\_\_.  **6.** Excess loads can cause the forklift to be \_\_\_\_\_\_\_ and tip over.  **10.** Pedestrians need to keep a \_\_\_\_\_\_ foot distance from forklifts.  **11.** Most forklifts steer from the \_\_\_\_\_.  **15.** Forklifts should be equipped with a \_\_\_\_\_\_ alarm to warn others. |