|  |  |
| --- | --- |
| Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

Preventing Forklift Accidents

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  | 1S |  E |  A |  T |  B |  E |  L |  T |  S |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  | 2O |  V |  E |  R |  H |  E |  A |  D |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  | 3B |  |  |  |  |  |  |  |
|  |  |  |  |  | 4P |  |  |  |  |  |  |  A |  |  | 5P |  |  |  |  |
|  |  |  |  |  |  E |  |  |  |  | 6T |  |  C |  |  |  A |  |  |  |  |
|  | 7I |  N |  S |  I |  D |  E |  |  | 8F |  O |  R |  K |  S |  | 9S |  L |  O |  W |  |
|  |  |  |  |  |  E |  |  |  |  |  P |  |  |  |  |  S |  |  |  |  |
|  |  |  |  |  |  S |  |  | 10F |  |  H |  |  |  |  |  E |  |  |  |  |
|  |  |  | 11R |  |  T |  | 12W |  I |  D |  E |  | 13H |  O |  R |  N |  |  |  |  |
|  |  |  |  E |  |  R |  |  |  V |  |  A |  |  |  |  |  G |  |  |  |  |
|  |  | 14B |  A |  L |  A |  N |  C |  E |  |  V |  |  |  |  |  E |  |  |  |  |
|  |  |  |  R |  |  I |  |  |  |  |  Y |  |  |  |  |  R |  |  |  |  |
|  |  |  |  |  |  N |  |  | 15B |  |  |  |  |  |  |  S |  |  |  |  |
|  |  |  |  |  | 16S |  T |  R |  A |  I |  G |  H |  T |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  C |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  K |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  U |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  | 17I |  N |  S |  P |  E |  C |  T |  E |  D |  |  |  |  |  |  |

|  |  |
| --- | --- |
| **Across****1.** Drivers should always wear \_\_\_\_\_\_.**2.** All rider forklifts must have an \_\_\_\_ guard to protect the operator from falling objects.**7.** The driver should keep hands, arms, and legs \_\_\_\_ in case of a tipover.**8.** No one should be allowed to stand or pass under the \_\_\_\_\_.**9.** Operators should \_\_\_\_\_\_ down and sound the horn at intersections and when entering the shop.**12.** The back of a forklift swings \_\_\_\_\_ on a turn.**13.** Drivers need to sound the \_\_\_\_\_ blind corners, doorways and aisles.**14.** Sharp or sudden turns can throw a forklift off \_\_\_\_\_\_\_.**16.** Forklifts should travel only \_\_\_\_ up and down a grade.**17.** Forklifts must be \_\_\_\_\_\_\_before each shift. | **Down****3.** Loads should be placed as far \_\_\_\_\_ as possible for extra stability.**4.** Almost one out of five fatal accidents kill other workers or \_\_\_\_\_.**5.** Drivers should never carry \_\_\_\_\_\_\_\_.**6.** Excess loads can cause the forklift to be \_\_\_\_\_\_\_ and tip over.**10.** Pedestrians need to keep a \_\_\_\_\_\_ foot distance from forklifts.**11.** Most forklifts steer from the \_\_\_\_\_.**15.** Forklifts should be equipped with a \_\_\_\_\_\_ alarm to warn others. |