|  |  |
| --- | --- |
| Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

Safety Crossword Puzzle

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | 1 |  |  |  |  | 2 |  |  |  |  |  |
| 3 |  |  |  |  |  |  |  |  |  |  |  | 4 |  |  |
|  |  |  |  |  |  | 5 |  |  |  |  |  |  |  |  |
|  |  | 6 |  |  |  |  |  |  |  |  |  |  | 7 |  |
|  |  |  |  | 8 |  |  |  |  |  |  |  |  |  | 9 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  | 10 |  |  | 11 |  |  |  |  |  |  |  |
|  |  |  | 12 |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 13 |  |  |  |  |  |  |  | 14 |  |  |  |  |  |  |
|  | 15 |  |  |  |  |  |  |  |  |  |  |  |  | 16 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 17 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  | 18 |  |  |  |  |  |  |  |  |  |  |  |
|  |  | 19 |  |  |  |  |  |  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| **Across**  **1.** Form that explains hazards of chemicals  **5.** Government agency established to enforce workplace safety rules  **8.** Direction forklift drivers should drive when carrying loads up an incline  **12.** Word used to correspond with the most toxic material  **13.** Number of required sections on an SDS  **14.** Safety glasses, gloves, earplugs, etc.  **15.** Safety Data sheets must be in this language  **17.** A process that allows the body to adjust to increased heat exposure  **18.** Stairway safety feature  **19.** A way toxic chemicals can enter your body | **Down**  **2.** Should never be used as a step stool  **3.** Fall arrest system is repuired when working at this height or more  **4.** Happens when the body can no longer control it's temperature  **6.** Area you aim a fire extinguisher at when putting out a fire  **7.** Responsible for providing you with personal protective equipment  **9.** Blockage of direct sunlight  **10.** All containers are required to have one  **11.** color on the NFPA marking system that implies flammability  **16.** Something forklift drivers should do when going in or out of a building |