|  |  |
| --- | --- |
| Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

Sewing Tools

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 1T |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  H |  |  |  |  |  | 2T |  |  |  |  |  |  |  |
|  |  | 3P |  I |  N |  K |  I |  N |  G |  S |  H |  E |  A |  R |  S |  |  |  |  |  |
|  |  |  |  |  |  |  M |  |  |  |  |  |  P |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  B |  |  |  |  |  |  E |  |  |  |  |  |  |  |
|  |  |  | 4N |  |  |  L |  |  |  | 5H |  |  M |  |  | 6T |  |  |  |  |
|  |  |  |  E |  |  |  E |  |  |  |  A |  |  E |  |  |  R |  |  |  | 7F |
|  | 8S |  |  C |  |  |  | 9I |  R |  O |  N |  |  A |  |  |  A |  |  |  |  A |
|  |  E |  |  K |  |  |  |  |  |  |  D |  |  S |  |  |  C |  |  |  |  B |
|  |  A |  |  L |  |  |  |  | 10P |  I |  N |  C |  U |  S |  H |  I |  O | 11N |  |  R |
|  |  M |  |  I |  |  |  |  |  |  |  E |  |  R |  |  |  N |  |  E |  |  I |
| 12F |  R |  E |  N |  C |  H |  C |  U |  R |  V |  E |  |  E |  |  |  G |  |  E |  |  C |
|  |  I |  |  E |  |  |  |  |  |  |  D |  |  |  |  |  W |  |  D |  |  S |
|  |  P |  |  |  |  |  | 13T |  A |  I |  L |  O |  R |  S |  C |  H |  A |  L |  K |  |
|  |  P |  |  |  |  |  |  |  |  |  E |  |  |  |  |  E |  |  E |  |  |
|  |  E |  |  |  |  |  |  |  |  |  |  |  |  |  |  E |  |  |  |  |
|  |  R |  |  |  | 14C |  H |  A |  L |  K |  P |  E |  N |  C |  I |  L |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  | 15T |  H |  R |  E |  A |  D |  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| **Across****3.** This is popular in zigzagging or scalloped edge or for seam finishes**9.** This tool is used to make fabric flat**10.** It holds the straight pins and needles while-working to prevent accidents**12.** What tool is used to shape the depth of the neckhole and armhole of the pattern**13.**  It is available in a range of colors and is Removed by brushing**14.** It is used to make fine lines on fabric. It has an erasing brush at one end.**15.** It is used in assembling or constructing the parts of the garment. | **Down****1.** small hard pitted cup worn for protection on the finger that pushes the needle in sewing.**2.** What kind of measuring tool is used for taking body measurement**4.** French curve is used for shaping**5.**  It aids in putting the thread to the needle.**6.** Works like a pizza cutter and can be used by left or right-handed sewers**7.** It is the cloth used in making garments.**8.** It is specifically designed for ripping out stitches from seams, either as a result of an error or during alterations. **11.**  Has an eye and is used to carry thread through the fabric to make stitches |