|  |  |
| --- | --- |
| Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

Technical Cross Word

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  | 1 |  |  |  |  |  | 2 |  |  | 3 |  |  |  |
|  |  | 4 |  |  |  |  |  |  |  |  |  | 5 |  |  |  |  |  | 6 |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  | 7 |  |  |  |  |  |  |  |  |
|  |  |  |  | 8 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  | 9 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  | 11 |  |  | 12 |  |  |  |  |  |  |  | 13 |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 14 |  |  |  |  |  | 15 |  | 16 |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  | 17 |  |  |  |  |  |  | 18 |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  | 19 |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 20 |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| **Across**  **4.** a conductor through which electricity enters or leaves a substance.  **5.**  a \_\_\_\_\_\_ is a network hardware device that modulates carriers  **8.** Device used to transfer electrical energy from one circuit to another  **9.** To much power into a battery  **12.** an electric cell in which the electrolyte is absorbed in a solid to form a paste, preventing spillage.  **14.**  carries out the instructions of a computer program by performing the basic arithmetic, logical, control and input/output (I/O) operations specified by the instructions  **16.** Voltage controlled device  **17.** A circuit with two or more paths  **19.** Set of wires that carries the electricity supply  **20.**  what is any set of instructions that tells the hardware what to do and how to do it. | **Down**  **1.**  \_\_\_\_\_\_\_\_\_\_\_\_\_terminal of MOSFET is similar to collector in BJT  **2.**  a computer \_\_\_\_\_\_ is a handheld device that detects two dimensional motion  **3.** protocol used for sending e-mail over the Internet using a set of commands that authenticate and direct the transfer of electronic mail  **6.** an automatic device for stopping the flow of current in an electric circuit as a safety measure.  **7.** A method of transmitting data in which data is sent out to all nodes on a network and is retrieved only by the intended recipient.  **10.** BJT acts as ON switch in \_\_\_\_\_\_\_\_\_\_region  **11.** Sending an email, posting photos on a social media site and using your webcam.  **13.** a conductor through which electricity enters or leaves an object, substance, or region.  **15.** you can hold data and files in a  **18.** BJT acts as ON switch in \_\_\_\_\_\_\_\_\_\_region |