|  |  |
| --- | --- |
| Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ |

Vocab Module Three

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  | 1 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  | 2 |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  | 3 |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  | 4 |  |  |  |  |  |  |  |  |  |  |  | 5 |
|  |  |  | 6 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  | 7 |  |  |  |  |  | 8 |  |  | 9 |  |  |  |  |  |
|  |  | 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |  | 11 |  |  |
|  | 12 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  | 13 |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  | 14 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | 15 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  | 16 |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  | 17 |  |  |  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| **Across****1.** an adjustable carpenters tool consisting of a steel rule that slides through an adjustable head**3.** the point where members or the edges of members are joined**10.** A hammer with a flat face that is used to strike cold chisels and punches**13.** A metal tool with a sharpened, beveled edge used to cut and shape wood**14.** a flat steel square commonly used in carpentry**15.** A pin, usually round, that fits into a corresponding hole to fasten or align two peices**16.** unit of measure used to describe the amount of pressure exerted to an object**17.** a tool used to remove nails | **Down****2.** a wrench with an opened and closed end**4.** To cut on a slant at an angle that is not a right angle (90 degrees) **5.** A square whos legs are fixed at a right angle**6.** describing a surface made smooth by using a tool called a plane**7.** perfectly vertical, the surface is at a right angle, to the horizon or floor and does not bow at the top or bottom**8.** A device such as a bolt, clasp, hook, or lock used to attach or secure one material to another**9.** Perfectly horizontal, completely flat. Also, a tool used to determine if an objects level**11.** A hammer with a flat striking face. The other end of the head is curved and divided into two claws to remove nails**12.** a wrench, usually double ended, that has a closed socket that fits over the head of a bolt |